[Version] 
Signature="$Windows NT$"
Class=Ports
ClassGuid={4D36E978-E325-11CE-BFC1-08002BE10318}
Provider=%MFGNAME%
DriverVer=20/02/2010,1.0.0000.0

[Manufacturer] 
%MFGNAME%=CDCDevice,NT,NTamd64

[DestinationDirs]
DefaultDestDir = 12

[CDCDevice.NT]
%USBSR0_DESCRIPTION%=DriverInstall,USB\VID_1EC4&PID_8004&REV_0100
%USBSR1_DESCRIPTION%=DriverInstall,USB\VID_1EC4&PID_8002&REV_0101
%USBSR2_DESCRIPTION%=DriverInstall,USB\VID_1EC4&PID_8024&REV_0100
%USBSR3_DESCRIPTION%=DriverInstall,USB\VID_1EC4&PID_8022&REV_0101
%USBSR4_DESCRIPTION%=DriverInstall,USB\VID_1EC4&PID_8026&REV_0101

[CDCDevice.NTamd64]
%USBSR0_DESCRIPTION%=DriverInstall,USB\VID_1EC4&PID_8004&REV_0100
%USBSR1_DESCRIPTION%=DriverInstall,USB\VID_1EC4&PID_8002&REV_0101
%USBSR2_DESCRIPTION%=DriverInstall,USB\VID_1EC4&PID_8024&REV_0100
%USBSR3_DESCRIPTION%=DriverInstall,USB\VID_1EC4&PID_8022&REV_0101
%USBSR4_DESCRIPTION%=DriverInstall,USB\VID_1EC4&PID_8026&REV_0101

[DriverInstall.NT]
CopyFiles=RiffBoxFiles
AddReg=DriverInstall.NT.AddReg

[DriverInstall.NT.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,riffbox32.sys
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[DestinationDirs]
RiffBoxFiles=12
DefaultDestDir = 12

[RiffBoxFiles]
riffbox32.sys,,,0x20

[DriverInstall.NT.Services]
AddService=riffbox, 0x00000002, DriverServiceInst

[DriverServiceInst]
DisplayName		=%SERVICE%
ServiceType		=1
StartType		=3
ErrorControl	=1
ServiceBinary	=%12%\riffbox32.sys 

[Strings]
MFGNAME = "RIFF BOX Limited (c), 2016"
USBSR0_DESCRIPTION = "RIFF BOX Control Port"
USBSR1_DESCRIPTION = "RIFF BOX Firmware Update Port"
USBSR2_DESCRIPTION = "RIFF BOX II Control Port"
USBSR3_DESCRIPTION = "RIFF BOX II Firmware Update Port"
USBSR4_DESCRIPTION = "RIFF BOX II SelfTest Port"
SERVICE = "RIFFBOX_2016"
